**Jaeger NXT as a tracker variant:**

**Straight-pull bolt-action rifle for walk-through shooting and tracking**

**The NXT has almost everything you need for this hunting niche: now enhanced with a short barrel and Tracker iSight system**

**The term ‘bull's eye’ is used colloquially to describe when something fits perfectly - this also applies to a hunting rifle that ideally covers a not-so-narrow range of applications. The Jaeger NXT Tracker is probably close to what is generally defined as the ‘ideal rifle for shooting and tracking’.**

Short, handy, robust, fast, variable - and safe. These are the characteristics that tracking and traversing shooters expect from the rifle they use to break through the thicket. The Jaeger NXT comes with a central dowry: The rifle is - unusually in this price range - a genuine hand cocking device that can be safely carried even in difficult terrain with an uncocked action. The rifle thus remains relaxed until shortly before the shot - an important safety advantage for fellow hunters, dogs and the shooter himself. A simple safety device is not enough, especially when stumbling, walking at the lowest speed and getting stuck are part of the job.

**Hand cocking: carry safely uncocked, shoot at lightning speed**

Nevertheless, the kickdown chamber handle can be used to get the rifle ready to fire at lightning speed: Simply push forwards and the system is cocked and ready to fire. With an additional chamber lock lever, the bolt handle can also be completely blocked if required. And the 5-round magazine is secured against loss as standard with a patented extra lock.

A further weighty argument for hunters who are experienced in undergrowth: the iSight system for variable sights takes into account the different needs of stand shooters, walk-through shooters and gun dog handlers in a single rifle.

**iSight and sling swivel system: super variable**

In the Tracker variant, the iSight system opens up all target-oriented options on the barrel: the front sight can be completely removed or mounted in a recessed position with a single screw (M3, hexagon socket). The muzzle thread (M15x1) can also be fitted with a standard silencer when the front sight is set back - this protects the hearing of man and dog when firing short shots with open sights. Anything is possible: The rifle can be used without open sights if the overbarrel silencer is screwed onto the muzzle thread. Advantage: Combined with red dot optics, nothing irritating protrudes into the line of sight.

**Short barrel and four sling swivel sockets**

Haenel has further perfected the rifle for the intended use with a special ‘support structure’ and a short barrel (470 mm barrel length): The front tracker sling swivel mount also utilises the muzzle thread; it is simply screwed on and then sits securely on the left. It corresponds with the sling swivel bushing on the left side of the buttstock, in which the push-button system is locked. The classic sling swivel sockets at the bottom of the fore-end and buttstock are retained and increase the options for engaging the push-button sling as required.

And some more data on handling: with the 19-millimeter semi-weighted barrel, the rifle has a short overall length of 99 centimeters. Combined with the robust wood compound stock (FSC-certified composite wood), this straight-pull repeater weighs around 3.1 kilograms unloaded. The rifle will be available at market launch in .308 Win. and 8x57IS calibers.

\*\*\*

**Technical data:**

**Haenel Jaeger NXT Tracker**

**Straight-pull bolt-action rifle with patented torsion lock and kickdown manual cocker via the bolt handle, 5+1 shot magazine with lock and i-Sight system.**

**Barrel:** 19 mm diameter

**Overall length:** 990 mm

**Barrel length:** 470 mm

**Caliber:** .308 Win. and 8x57IS

**Total weight:** approx. 3,1 kg

**Sight:** i-Sight system, with muzzle thread (M15x1) and muzzle-cap

**PUBLISHER**

C.G. Haenel GmbH

Schützenstraße 26

D-98527 Suhl

Phone: +49 (0)3681 854 0

Fax: +49 (0)3681 854 203

Email: jean.freyeisen@cg-haenel.de

www.cg-haenel.de

**PRESS CONTACT**

id pool GmbH

Spinnerei 2

D-71522 Backnang

Phone: +49 (0) 1727415612

Email: haenel@id-pool.de

www.id-pool.de