**Perfect Fit: Jaeger NXT Stock Now Features Height Adjustment – Even in Wood**

**Enhanced Adjustability: C.G. Haenel introduces a height-adjustable cheek piece with the push of a button, enhancing their wood-compound stock.**

The elegant and ergonomic wooden stock of the Jaeger NXT bolt-action rifle has received a significant functional upgrade. With a height-adjustable cheek rest, wooden stock enthusiasts can now acquire targets faster, bringing the performance of the wood-compound stock closer to that of composite plastic alternatives.

Launched in 2021, the Jaeger NXT featured a robust wooden stock design. In 2023, Haenel added a composite plastic option, known for its versatility and superior adjustability in its price range. This has become a must-have for many, especially in the Jaeger NXT, an all-around rifle perfect for driven hunts. The adjustable cheek rest aids quick scope alignment and ensures a consistent shooting position for every hunt.

Following the success of this feature in the composite version, demand grew for similar functionality in the wooden stock. Haenel has now answered the call with the **Jaeger NXT Adjustable**, featuring a height-adjustable cheek rest operated by a simple push-button mechanism.

**Laminated Wood with Superior Durability**

The wood-compound stock incorporates technology from yacht building, with a striking grain pattern that rivals the beauty of fine wooden stocks. The laminated wood, sourced from fast-growing birch, is FSC-certified, ensuring sustainability – with no ancient highland walnut trees used here.

**Wooden Stock Matches Rifle’s Precision**

The ergonomic quality of the stock complements the straight-pull bolt-action design of the Jaeger NXT. Its torsion lock mechanism, powered by a bevel gear and secured with locking lugs, provides smooth and reliable operation. The bolt handle not only cycles the action, but also serves as a cocking mechanism. Unlike traditional cocking devices that require considerable finger strength, the Jaeger NXT’s kickdown bolt handle uses leverage for easy, quiet cocking, cycling, and de-cocking, all without repositioning your hand.

**Technical data:**

**Haenel Jaeger NXT Adjustable**

**Straight-pull bolt-action rifle with patented torsion lock and kickdown manual cocker via the bolt handle, adjustable FSC wood-compound stock, 5+1 shot magazine with lock and i-Sight system.**

**Barrel contour:** 18 mm diameter

**Barrel length:** 520 mm / Magnum 610 mm  
**Caliber:** .308 Win.

.30-06 Spring.

8x57 IS

.300 Win. Mag.

**Stock versions:** Adjustable with guided and push-button-released  
cheek piece in black.

**Overall length:** 1,045 mm (standard calibers)

**Total weight:** 3.2 kg

\* \* \*

**PUBLISHER**

C.G. Haenel GmbH

Schützenstraße 26

D-98527 Suhl

Phone: +49 (0)3681 854 0

Fax: +49 (0)3681 854 203

Email: jean.freyeisen@cg-haenel.de

www.cg-haenel.de

**PRESS CONTACT**

id pool GmbH

Spinnerei 2

D-71522 Backnang

Phone: +49 (0) 1727415612

Email: haenel@id-pool.de

www.id-pool.de